Classification of time signals by CNN using spectrogram

Thanh Toan, Truong: email

Hoang Hai, Pham: hhoang@student.fra-uas.de

Phan Bao Viet, Nguyen: email

Riyad-Ul-Islam: riyad-ul.islam@stud.fra-uas.de

Link to project:

*Abstract*—This electronic document is a “live” template and already defines the components of your paper [title, text, heads, etc.] in its style sheet. *\*CRITICAL: Do Not Use Symbols, Special Characters, Footnotes, or Math in Paper Title or Abstract*. (*Abstract*)

Keywords—component, formatting, style, styling, insert (key words)

# Introduction

## Literature Review

(Viet Nguyen)

# Methodology

## Overview

## Gabor Transform and Creation of Spectrogram

(Toan Truong)

## Convolutional Neural Network configuration

(Toan Truong)

## Graphical User Interface GUI

(Hai Pham)

A user-friendly GUI was created to implement the experiment of Gabor transform as well as CNN classifier. The app is named “GUI.mlapp”. The figure below shows the GUI of this project.

[FIGURE OF GUI HERE]

Figure [NUMBER] shows the GUI is divided into three sections:

* The first section is located at the top left corner of the frame. This one is used for loading training data files and create spectrograms for each sample in the training data.
* The section which is used for training and validating the data is right under the first section.
* The last section is situated at the left panel of the GUI. This section indicates the predicted results of test data files.

The following is a short manual instruction in order to run the GUI application:

* Step 1: First and foremost, user needs to load the training files by pressing the button “Browse File” as shown in figure [NUMBER] -> FIGURE WITH BROWSE FILE BUTTON RED . Currently, the training dataset includes three files “Data Object 1”, “Data Object 2”, “Data Object 3” which are located inside folder “dataset”. User can choose one file, two files or three file files at the same time for training purpose. After choosing training files, the names of all chosen files are illustrated in the table to help the user can check it again.
* Step 2: Press the button “Create Spectrogram” to generate all spectrograms from the “Data Object” files. All the images are stored in folder “trainingData”, which is created automatically by Matlab. There is a LED in the lower area of the “Create Spectrogram” button to illustrate status of the process. As depicted in the figure [NUMBER] -> FIGURE WITH LED ORANGE AND CREATE SPECTROGRAM, the LED shows orange and the status indicates “Processing” while the program is running. After creating spectrograms, the LED changes to green and the status also alternates to “Finished”.

# Experiment

## Experiment’s result

(Riyad)

## Result on Given Test data

(Riyad)

# Conclusion

# Further Development

(Toan Truong)

##### References

1. G. Eason, B. Noble, and I. N. Sneddon, “On certain integrals of Lipschitz-Hankel type involving products of Bessel functions,” Phil. Trans. Roy. Soc. London, vol. A247, pp. 529–551, April 1955. *(references)*
2. J. Clerk Maxwell, A Treatise on Electricity and Magnetism, 3rd ed., vol. 2. Oxford: Clarendon, 1892, pp.68–73.
3. I. S. Jacobs and C. P. Bean, “Fine particles, thin films and exchange anisotropy,” in Magnetism, vol. III, G. T. Rado and H. Suhl, Eds. New York: Academic, 1963, pp. 271–350.
4. K. Elissa, “Title of paper if known,” unpublished.
5. R. Nicole, “Title of paper with only first word capitalized,” J. Name Stand. Abbrev., in press.
6. Y. Yorozu, M. Hirano, K. Oka, and Y. Tagawa, “Electron spectroscopy studies on magneto-optical media and plastic substrate interface,” IEEE Transl. J. Magn. Japan, vol. 2, pp. 740–741, August 1987 [Digests 9th Annual Conf. Magnetics Japan, p. 301, 1982].
7. M. Young, The Technical Writer’s Handbook. Mill Valley, CA: University Science, 1989.